D. Directory Migration (DM_*)
Eight adapter interfaces for every infrastructure service AD was holding together
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D. Directory Migration (DM_*)
Active Directory was the implicit governance anchor for eleven categories of infrastructure objects. When AD goes away, each must be migrated to a modern equivalent with governance preserved. DM_* adapters define the interface; vendor implementations plug in underneath.
Leaves
	ID
	Adapter
	Status

	D.1
	IPAM Adapter — DM_010
	Source present

	D.2
	DNS Adapter — DM_015
	⚠ gap — not in registry

	D.3
	DHCP Adapter — DM_016
	⚠ gap

	D.4
	PKI / ADCS Adapter — DM_020
	Source present

	D.5
	RADIUS / NPS Adapter — DM_030
	Source present

	D.6
	LDAP Proxy Adapter — DM_040
	Source present

	D.7
	Sync Engine Adapter — DM_050
	Source present

	D.8
	Device Management Adapter — DM_060
	Source present

	D.9
	NTP Adapter — DM_070
	Source present

	D.10
	DFS Adapter — DM_080
	Source present

	D.11
	SPN / App Registration — DM_085
	⚠ gap

	D.12
	Trust Relationship — DM_090
	⚠ gap


Canon surface: modernization/directory-migration.qmd
Canon Phase Mapping Requirement (the program decision)
Every leaf in this subcategory — DNS, PKI, RADIUS, LDAP, DHCP, Sync Engine, Device Management, NTP, DFS, and the SPN / Trust gap-fillers — MUST publish a Canon Phase Mapping table at the top of its operational guide, mapping the guide’s phases to the canonical six-phase Directory Migration model (Discover → Normalize → Map → Migrate → Validate → Decommission). Per [the program decision], this requirement applies to every existing and future adapter guide in this taxonomy.
Reference implementations: DNS Modernization (11→6 mapping) and PKI Modernization (6→6 mapping). Contributor guidance is in [src/fmp/modernization/directory-migration/README.md] under “Adding a New Adapter Migration Guide”.
